New check valve
with redundant sealing

Klingenberg, August 2020. The new model CV check valve from WIKA is designed for a wide range of applications in the process industry. Its sealing system with a self-centering piston reliably prevents backflow of liquid and gaseous media.

The reliability of the new instrumentation valve is mainly due to its redundant sealing, consisting of an O-ring and a metal cone. Its leak tightness has been tested in accordance with BS6755/ISO 5208 leakage rate A. The solid-machined, robust design of the model CV ensures high repeatability and a long service life, even in heavy-duty applications. The pressurized parts correspond to the safety factor of 4:1.

For the new check valve, WIKA offers an application-specific assembly with a measuring instrument. Such an instrument hook-up is delivered ready-to-install and leak tested.

Number of characters: 797

Key word: CV

**Manufacturer:**

WIKA Alexander Wiegand SE & Co. KG

Alexander-Wiegand-Straße 30

63911 Klingenberg/Germany

Tel. +49 9372 132-0

Fax +49 9372 132-406

vertrieb@wika.com

[www.wika.de](http://www.wika.de/)

**WIKA company photograph:**



**Typ: CV**

**Edited by:**

WIKA Alexander Wiegand SE & Co. KG

André Habel Nunes

Marketing Services

Alexander-Wiegand-Straße 30

63911 Klingenberg/Germany

Tel. +49 9372 132-8010

Fax +49 9372 132-8008010

andre.habel-nunes@wika.com

[www.wika.de](http://www.wika.de/)

WIKA press release